{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["ANT-001-0001D"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ANT-001-0001D","index":0,"n_rows":22,"n_cols":19,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"ANT-001-0001D",{"$nulls":7},"販売店情報"]
[{"$nulls":7},"パーツメーカ情報",null,null,null,"参考価格",null,null,null,"参考価格",null,null,"備考"]
["項","品名","リファレンス","数量","実装数","定格・仕様","パッケージ","メーカー","品番","販売店1","販売店品番1","最小発注","100台分","販売店2","販売店品番2","最小発注","100台分","ロスト率 (%)"]
["1","チップアンテナ","A1","1","1","2.4GHz ISM","1608","PULSE ELECTRONICS CORPORATION","W3008C","Digi-Key","553-1674-1-ND"]
["2","セラミックコンデンサ","C1,C3,C4,C9.C14.C15,C16,C17,C18,C24","10","10","0.1uF","1005","村田製作所","GRM155R71C104KA88D","Digi-Key","490-3261-1-ND"]
["3","セラミックコンデンサ","C2,C8","2","2","0.033uF","1005","TDK Corporation","C1005X7R1C333K","Digi-Key","445-4947-1-ND"]
["4","セラミックコンデンサ","C5","1","1","1.5pF","1005","TDK Corporation","C1005C0G1H1R5C","Digi-Key","445-4859-1-ND"]
["5","セラミックコンデンサ","C6","1","1","1pF","1005","TDK Corporation","C1005C0G1H010C","Digi-Key","445-4855-1-ND"]
["6","セラミックコンデンサ","C7","1","1","2200pF","1005","Yageo","GRM155R71H222KA01D","Digi-Key","490-1305-1-ND"]
["7","セラミックコンデンサ","C10,C11,C12,C13","4","4","15pF","1005","Yageo","CC0402JRNP09BN150","Digi-Key","311-1017-1-ND"]
["8","セラミックコンデンサ","C25","1","0","DNI","1005"]
["9","スイッチ付RFコネクタ","J1","1","1","SWF","2.5x2.5","村田製作所","MM8130-2600RA2","Digi-Key","490-4981-1-ND"]
["10","ピンヘッダ","J2","1","1","10 x 2列"]
["11","チップインダクタ","L1","1","1","4.7nH","1005","Panasonic ECG","ELJ-RF4N7ZFB","Digi-Key","PCD1906CT-ND"]
["12","チップインダクタ","L2,L3","2","2","6.8nH","1005","Panasonic ECG","ELJ-RF6N8ZFB","Digi-Key","PCD1908CT-ND"]
["13","EIA574 コネクタ","P1","1","1","EIA-574 MALE","EIA574","TE Connectivity","1734351-1","Digi-Key","A35105-ND"]
["14","チップ抵抗","R1,R2,R3,R4,R5,R6,R7,R17","8","8","22kΩ","1005","Yageo","RC0402FR-0722KL","Digi-Key","311-22.0KLRCT-ND"]
["15","チップ抵抗","R18,R19,R20","3","0","0Ω","1608"]
["16","ANTチップ","U1","1","1","nRF24PA2-8CH","QFN-32","NORDIC","nRF24AP2-8CHQ32"]
["17","シリアルドライバ","U2","1","1","MAX3232","TSSOP-16","Texas Instruments","MAX3232IPWR","Digi-Key","296-13100-1-ND"]
["18","水晶発振子","X1","1","1","32768Hz ±50ppm以内","ABS10","Abracon Corporation","ABS10-32.768KHZ-9-T","Digi-Key","535-9538-1-ND"]
["19","水晶発振子","X2","1","1","16MHz ±50ppm以内","ECS160","ECS Inc","ECS-160-9-42-CKM-TR","Digi-Key","XC1611CT-ND"]