{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["bc10-001-0002_bom"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"bc10-001-0002_bom","index":0,"n_rows":107,"n_cols":17,"rows_kept":107,"cut":false,"hidden":false,"merged":[[1,11,1,12],[1,15,1,16]],"flags":["formulas_cached_only"]}
[{"$nulls":7},"Component Maker\n Information",null,"Retailer Information"]
[{"$nulls":11},"Price (¥:Reference)",null,null,null,"Price (Reference)"]
["Item #","Type","Reference","Quantity","# of Mounted ","Description","Package","Maker","Product Number","Retailer1","Part Number @Retailer1","@mini  number\n Unit per order ","@100 units","Retailar2","Part Number @Retailer2","@mini  number unit","@100 units"]
[1,"Chip Antenna","ANT1",1,"1","GPS_ANT",null,"JOHANSON TECHNOLOGY","1575AT43A40","sparkfun electronics","sku: GPS-09131",1.5,1.2]
[2,"Battery Holder","BT1",1,"1","BATTERY HOLDER",null,"Memory Protection Devices Inc","BU1632SM-JJ-GTR","Digi-Key","BU1632SM-JJ-GCT-ND",65,57.3]
["3","Ceramic Capacitor","C174",1,"1","15pF","0603","Murata","GRM0337U1H150JD01D","Digi-Key","490-3883-1-ND",4.6,2.73]
["4","Ceramic Capacitor","C95,C96",2,"2","22pF","0603","Murata","GRM0335C1E220JD01D","Digi-Key","490-1253-1-ND",2.3,1.37]
["5","Ceramic Capacitor","C23,C24,C85,C86,C93,C94,C165","7","7","47pF","0603","Murata","GRM0335C1E470JD01D","Digi-Key","490-1256-1-ND",2.3,0.788]
["6","Ceramic Capacitor","C77,C83,C84,C87,C88,C89,C90,C97",8,"8","100PF","0603","Murata","GRM033R71E101KA01D","Digi-Key","490-3172-1-ND",2.3,0.788]
["7","Ceramic Capacitor","C8,C188",2,"2","470pF","0603","Murata","GRM033R71E471KA01D","Digi-Key","490-3180-1-ND",2.3,1.37]
["8","Ceramic Capacitor","C170,C171,C213,C215","4","4","0.01uF","0603","Murata","GRM033R71A103KA01D","Digi-Key","490-3194-1-ND",2.3,1.37]
["9","Ceramic Capacitor","C2,C14,C18,C20,C21,C22,C25,C26,C28,C29,C32,C33,C34,C35,C36,C37,C38,C39,C40,C41,C42,C43,C44,C45,C47,C48,C49,C50,C51,C52,C54,C55,C56,C58,C59,C60,C61,C62,C63,C64,C65,C66,C69,C74,C75,C76,C78,C91,C92,C101,C104,C111,C126,C131,C133,C135,C137,C140,C141,C142,C143,C144,C145,C146,C147,C148,C149,C150,C151,C152,C154,C156,C157,C181,C185,C191,C193,C195,C196,C198,C199,C200,C201,C202,C203,C204,C205,C206,C207,C208,C209,C216","92","92","0.1uF","0603","Murata","GRM033R60J104ME19D","Digi-Key","490-5404-1-ND",3.6,0.6006]
["10","Ceramic Capacitor","C67,C68,C173",3,"3","0.22uF","1005","Murata","GRM155R61A224KE19D","Digi-Key","490-3910-1-ND",5.8,3.41]
["11","Ceramic Capacitor","C70,C72,C73,C82,C98,C102,C103,C107,C108,C109,C110,C114,C116,C117,C118,C119,C120,C121,C122,C124,C125,C128,C129,C158,C159,C160,C161,C162,C163,C164,C175,C177,C178,C179,C180,C186,C189,C190,C194",39,"39","1uF","1608","TAIYO YUDEN","LMK107BJ105KA-T","Digi-Key","587-1242-1-ND",5.8,1.379]
["12","Ceramic Capacitor","C100,C115","2","2","2.2uF","1608","TAIYO YUDEN","LMK107BJ225KA-T","Digi-Key","587-1253-1-ND",16.5,9.76]
["13","Ceramic Capacitor","C7,C9,C27,C30,C31,C46,C53,C57,C71,C79,C99,C132,C134,C138,C153,C155,C167,C168,C169,C172,C182,C183,C184,C187,C192,C210,C211,C212,C214","29","29","4.7uF","2012","TAIYO YUDEN","LMK212BJ475KD-T","Digi-Key","587-1297-1-ND",25.3,5.986]
["14","Ceramic Capacitor","C15,C176",2,"2","22uF","2012","TAIYO YUDEN","LMK212BJ226MG-T","Digi-Key","587-1958-1-ND",48,42.04]
["15","Ceramic Capacitor","C105,C106,C112,C113,C123,C127","6","6","10uF","2012","TAIYO YUDEN","LMK212BJ106KG-T","Digi-Key","587-1300-1-ND",27.5,6.507]
["16","Tantalum Capacitor","C16,C17,C139,C197",4,"4","10uF","3216-16","ROHM","TCA1A106M8R","Digi-Key","511-1463-1-ND",33,24.72]
["17","Ceramic Capacitor","C80,C81",2,"2","47uF","3216","TAIYO YUDEN","LMK316BJ476ML-T","Digi-Key","587-1780-1-ND",198.2,117.12]
["18","Tantalum Capacitor","C130",1,"1","100uf","7343-28","Nichicon","F931A107MNC","Digi-Key","493-2353-1-ND",133,87.54]
["19","Tantalum Capacitor","C10",1,"1","150uF","7343-28","Nichicon","F931A157MNC","Digi-Key","493-2355-1-ND",158,104.38]
["21","Green LED","D10,D11,D12,D17,D21,D22,D23,D24,D25,D26,D27,D28","12","12","LG L29K-G2J1-24-Z","1608","OSRAM Opto Semiconductors Inc","LG L29K-G2J1-24-Z","Digi-Key","475-2709-1-ND",16,8.752]
["22","Diode","D6,D7,D8,D9",4,"4","PGB1010603MR","1608","Littelfuse Inc","PGB1010603MR","Digi-Key","F2594CT-ND",86,66.19]
["23","Diode","D13,D14,D15,D16",4,"4","DIO_V5.5MLA0603","1608","Littelfuse Inc","V5.5MLA0603H","Digi-Key","F2214CT-ND",47,36]
["24","Schottky Barrier Diode","D18,D19,D20",3,"3","MBRM120","Powermite","ON Semiconductor","MBRM120ET1G","Digi-Key","MBRM120ET1GOSCT-ND",57,25.788]
["25","AMOLED Connector  ","JP1",1,"1","FH26-71S","FH26-71S","Hirose Electric Co Ltd","FH26-71S-0.3SHW(05)","Digi-Key","HFQ371CT-ND",412,255.86]
["27","6-pin Connector","J3","1","1","DF13A-6","DF13A-6","Hirose Electric Co Ltd","DF13A-6P-1.25H(20)","Digi-Key","H3371-ND",72,42.79]
["28","microSD slot","J5",1,"1","3M 2908-05WB","dm3at","3M","2908-05WB-MG","Digi-Key","3M5607CT-ND",123,93.31]
["29","SD Slot","J6",1,"1","DM1","dm1","Hirose Electric Co Ltd","DM1AA-SF-PEJ(21)","Digi-Key","HR845CT-ND",397,246.85]
["30","iPod Connector","J7",1,"1","iPod30","ipod-30","DAWEI PRECISION ","iPOD-CNN30P","sparkfun electronics","sku: DEV-08035"]
["31","Camera Connector","J8",1,"1","X2A 5M AF","X2A_5M_AF","Panasonic Electric Works","AXK724147G","Digi-Key","255-2535-1-ND",272,188.89]
["32","Expansion Connector ","J9,J10",2,"2","24 5078 030 510 861+","245708030","KYOCERA ELCO","24 5078 030 510 861+","chip 1 stop","145078030510861+"]
["34","Inductor","L2,L3",2,"2","3.3uH","1608","Taiyo Yuden","LK16083R3K-T","Digi-Key","587-1584-1-ND",13.7,10.93]
["35","Inductor","L4,L6",2,"2","1uH, 2A",null,"TDK Corporation","VLF3012ST-1R0N2R0","Digi-Key","445-4199-1-ND",122,94.59]
["36","Inductor","L5",1,"1","1uH",null,"TDK Corporation","CPL2512T1R0M","Digi-Key","445-4170-1-ND",60,40.04]
["37","Inductor","L7,L8,L9",3,"3","FERRITE, MMZ1608R301A",null,"TDK Corporation","MMZ1608R301A","Digi-Key","445-2171-1-ND",5.3,3.512]
["38","Inductor","L10,L11",2,"2","B82462G4472M",null,"EPCOS Inc","B82462G4472M","Digi-Key","495-1997-1-ND",190,142.38]
["39","miniUSB TypeAB Connector","P1",1,"1","56579-0576 ",null,"Molex","565790-576","Digi-Key","WM17122CT-ND",281,183.61,"chip1stop",565790576,296,149]
["40","bc10 JTAG Connector","P2",1,"1","DF13C-14P-1.25V",null,"Hirose Electric Co Ltd","DF13C-14P-1.25V(20)","Digi-Key","H3430-ND",133,78.83]
["41","Stereo Mini-Jack","P3",1,"1","PHONOJACK STEREO-R",null,"CUI Inc","SJ-3523-SMT","Digi-Key","CP-3523SJCT-ND",87,57.86]
["42","USB TypeA Connector","P4",1,"1","USB-A Conn. - 87520-xx1xx",null,"Mill-Max Manufacturing Corp.","896-43-004-00-000000","Digi-Key","ED90065-ND",159,109.91]
["43","HDMI Connector","P5",1,"1","HDMI_Conn",null,"FCI","10029449-001RLF","Digi-Key","609-1010-1-ND",99,54.35]
["44","FET","Q2",1,"1","Si2323DS","SOT23-3","Vishay/Siliconix","SI2323DS-T1-E3","Digi-Key","SI2323DS-T1-E3CT-ND",133,89.99,"chip1stop","SI2323DS-T1-GE3",392,113]
["45","Single in Line Resistor","RP1,RP2,RP3,RP4",4,"4",10,null,"Rohm Semiconductor","MNR18E0APJ100","Digi-Key","MNR18100CT-ND",9.5,7.44]
["46","Polyswitch","RT1",1,"1","MICROSMD010F-2",null,"Tyco Electronics ","MICROSMD010F-2","Digi-Key","MICROSMD010FCT-ND",54,42.67]
["47","Chip Resistor","R65,R80,R90","3","3",0,"1005","Panasonic","ERJ-2GE0R00X","Digi-Key","P0.0JCT-ND",8.1,2.515]
["48","Chip Resistor","R56,R139,R140","3","3",0,"1608","Panasonic","ERJ-3GEY0R00V","Digi-Key","P0.0GCT-ND",7.1,2.195]
["50","Chip Resistor","R44,R45,R46","3","0","0,DNI","1005"]
["50","Chip Resistor","R93,R94,R131","3","0","0,DNI","1608","Panasonic","ERJ-3GEY0R00V","Digi-Key","P0.0GCT-ND",0,0]
["51","Chip Resistor","R92","1","0","0,DNI","2012","Panasonic","ERJ-6GEY0R00V","Digi-Key","P0.0ACT-ND",0,0]
["52","Chip Resistor","R11",1,"1",0.1,"2012","ROHM","MCR10EZHFLR100","Digi-Key","RHM.10MCT-ND",14.1,10.02]
["53","Chip Resistor","R17,R47,R48,R55,R57,R59,R70,R144","8","8",33,"1005","ROHM","MCR01MZPF33R0","Digi-Key","RHM33.0LCT-ND",8.2,2.54]
["54","Chip Resistor","R117",1,"1",100,1005,"ROHM","MCR01MZPF1000","Digi-Key","RHM100LCT-ND",8.2,4.42]
["56","Chip Resistor","R23",1,"1",470,"1005","Yageo","RC0402FR-07470RL","Digi-Key","311-470LRCT-ND",6.7,3.62]
["57","Chip Resistor","R22,R68",2,"0","470, DNI","1005","Yageo","RC0402FR-07470RL","Digi-Key","311-470LRCT-ND",0,0]
["58","Chip Resistor","R98",1,"1",510,"1005","ROHM","MCR01MZPF5100","Digi-Key","RHM510LCT-ND",8.2,4.42]
["59","Chip Resistor","R99,R102,R113",3,"3","1K","1005","ROHM","MCR01MZPF1001","Digi-Key","RHM1.00KLCT-ND",8.2,2.54]
["60","Chip Resistor","R16",1,"1","1k","1608","panasonic","ERJ-3EKF1001V","Digi-Key","P1.00KHCT-ND",7.3,3.92,"chip1stop","ERJ-3EKF1001V",30,24]
["61","Chip Resistor","R106,R107,R108",3,"0","1K, DNI","1608","panasonic","ERJ-3EKF1001V","Digi-Key","P1.00KHCT-ND",0,0]
["62","Chip Resistor","R15,R62,R76,R78,R120,R121,R122,R123,R124,R125,R126,R127,R129,R130","14","14","1.5k","1005","ROHM","MCR01MZPF1501","Digi-Key","RHM1.50KLCT-ND",8.2,1.73]
["63","Chip Resistor","R32,R33",2,"2","1.65K","1005","panasonic","ERJ-2RKF1651X","Digi-Key","P1.65KLCT-ND",9.8,3.045]
["64","Chip Resistor","R77,R79",2,"2","2.2k","1005","Yageo","RC0402FR-072K2L","Digi-Key","311-2.20KLRCT-ND",6.7,2.085,"Digi-Key","RHM2.20KLTR-ND"]
["65","Chip Resistor","R145",1,"1","2.7k","1005","Yageo","RC0402FR-072K7L","Digi-Key","311-2.70KLRCT-ND",6.7,3.62]
["66","Chip Resistor","R18,R19,R20,R21,R54,R58,R60,R100,R103,R109,R141,R142,R143,R147,R149,R150",16,"16","4.7K","1005","Panasonic","ERJ-2RKF4701X","Digi-Key","P4.70KLCT-ND",9.8,2.076]
["67","Chip Resistor","R89,R91","2","0","4.7k, DNI","1005","Panasonic","ERJ-2RKF4701X","Digi-Key","P4.70KLCT-ND",0,0]
["66","Chip Resistor","R136,R138","2","0","4.7K, DNI","1608"]
["69","Chip Resistor","R66,R96",2,"2","8.06k","1005","ROHM","MCR01MZPF8061","Digi-Key","RHM8.06KLCT-ND",8.2,2.54]
["70","Chip Resistor","R95",1,"1","8.45K","1005","panasonic ECG","ERJ-2RKF8451X","Digi-Key","P8.45KLCT-ND",9.8,5.3]
["71","Chip Resistor","R24,R25,R31,R38,R41,R42,R43,R51,R52,R53,R61,R63,R64,R67,R69,R75,R81,R82,R83,R84,R85,R86,R87,R88,R97,R101,R104,R105,R118,R119,R128,R132,R133,R134,R135,R146,R151","37","37","10k","1005","ROHM","MCR01MZPF1002","Digi-Key","RHM10.0KLCT-ND",8.2,1.73]
["72","Chip Resistor","R34,R37",2,"2","10k","1608","panasonic","ERJ-3EKF1002V","Digi-Key","P10.0KHCT-ND",7.3,2.255]
["73","Chip Resistor","R35,R36",2,"0","10k, DNI","1608","panasonic","ERJ-3EKF1002V","Digi-Key","P10.0KHCT-ND",0,0]
["74","Chip Resistor","R49,R50",2,"2","12k","1608","panasonic","ERJ-3EKF1202V","Digi-Key","P12.0KHCT-ND",7.3,2.25]
["75","Chip Resistor","R114","1","1","20k","1005","ROHM","MCR01MZPF2002","Digi-Key","RHM20.0KLCT-ND",8.2,2.54]
["76","Chip Resistor","R14",1,"1","22.6k","1608","panasonic","ERJ-3EKF2262V","Digi-Key","P22.6KHCT-ND",7.3,3.92]
["77","Chip Resistor","R12",1,"1","56.2k","1608","panasonic","ERJ-3EKF5622V","Digi-Key","P56.2KHCT-ND",7.3,3.92]
["78","Chip Resistor","R26,R27,R28,R29,R30,R115,R137,R148","8","8","100K","1005","ROHM","MCR01MZPF1003","Digi-Key","RHM100KLCT-ND",8.2,2.54]
["79","Chip Resistor","R112",1,"1","118k","1005","panasonic","ERJ-2RKF1183X","Digi-Key","P118KLCT-ND",9.8,5.3]
["80","Chip Resistor","R111",1,"1","390k","1005","panasonic","ERJ-2RKF3903X","Digi-Key","P390KLCT-ND",9.8,5.3]
["81","Chip Resistor","R116",1,"1","392k","1005","panasonic","ERJ-2RKF3923X","Digi-Key","P392KLCT-ND",9.8,5.3]
["82","Power Supply Switch","S1",1,"1","SW_SS3",null,"NKK Switches","SS3-12SAH4","chip 1 stop","SS3-12SAH4",330,173,"NKK Switches","SS3-12SAH4"]
["83","Mini Push Button Switch","S2,S3",2,"2","B3F-1000",null,"Panasonic","EVQPLHA15","Shoyodenko.Co.Ltd","EVQPLHA15"]
["84","Test Point 1","TP1,TP2",2,"0","TESTPT1"]
["85","Test Point 2","TP4,TP5,TP6,TP7,TP8,TP9,TP10,TP11,TP12,TP13,TP14,TP15,TP16,TP17,TP18,TP19,TP20,TP21,TP22,TP23,TP24,TP25,TP26,TP27,TP28,TP29,TP30,TP31,TP33,TP42,TP43,TP44,TP45,TP46","34","0","TESTPT1",null,"(The pattern is only printed\n on PCB)","(The pattern is only printed \non PCB)"]
["86","OMAP3530 CPU","U3",1,"1","OMAP3530DCBB","BGA CBB515","Texas Instruments","OMAP 3530","Tokyo Electron Device","OMAP3530"]
["87","Non-Inverse Dual Buffer/Driver","U4",1,"1","SN74LVC2G07DCKR","SOT(SC-70) - DCK","Texas Instruments","SN74LVC2G07DCKR","Digi-Key","296-13495-1-ND",66,39.64]
["88","Companion Chip","U5",1,"1","FBGA209_15-74_280x280","BGA ZXN-209","Texas Instruments","TPS65950BZXNR","Digi-Key","296-24096-1-ND",1194,900.9]
["90","LDO Power Supply IC","U7",1,"1","MIC5219-3.3YM5","SOT23-5","Micrel Inc","MIC5219-3.3YM5 TR","Digi-Key","576-1281-1-ND",170,102.1]
["93","Power Supply IC","U10",1,"1","TPS73701_DCQ6","DCQ SOT233","Texas Instruments","TPS73701DCQ","Digi-Key","296-19481-5-ND",202,146.4]
["94","Power Supply IC","U11",1,"1","TPS2061 (DGN)","DGN","Texas Instruments","TPS2061DGNR","Digi-Key","296-17225-1-ND",245,171.67]
["95","USB PHY Driver","U12",1,"1","USB3322C-GL-TR","USB3322C-GL-TR","SMSC","USB3322C-GL-TR","chip 1 stop","USB3322C-GL-TR",723,260]
["96","Level Convertor ","U13,U15,U17",3,"3","TXS0102 (DCU)","DCU VSSOP-8","Texas Instruments","TXS0102DCUR","Digi-Key","296-21931-1-ND",125,77.628]
["97","DVI Transceiver","U14",1,"1","TFP410","TQFP-64","Texas Instruments","TFP410PAP","Digi-Key","296-12666-ND",751,555.56]
["98","Touchscreen Controller","U16",1,"1","TSC2003IPWR","TSSOP-16","Texas Instruments","TSC2003IPW","Digi-Key","296-14340-1-ND",676,495.5]
["99","DCDC Rectifier","U18",1,"1","TPS65131","QFN-24","Texas Instruments","TPS65131RGET","chip 1 stop","TPS65131RGET",1280,463,"Digi-Key","TPS65131RGET",736,539.54]
["100","LDO Power Supply IC","U19",1,"1","MIC5219-2.8YM5","SOT23-5","Micrel Inc","MIC5219-2.8YM5 TR","Digi-Key","576-2762-1-ND",170,102.1]
["101","LDO Power Supply IC","U20",1,"1","MIC5258-1.2YM5","SOT23-5","Micrel Inc","MIC5258-1.2YM5 TR","Digi-Key","576-2828-1-ND",105,70.07]
["102","20ch GPS Module","U21",1,"1","MN5010",null,"MicroModular Technologies","MN5010HS","SemiconductorStore.com","MN5010HS-TS"]
["103","6-axis Motion Sensor","U22",1,"1","AMI602","LGA20","AICHI STEEL","AMI602","Tokyo Electron Device","AMI602"]
["104","Hex Inverter buffer/driver","U23,U24",2,"2","SN74LVC06A","TSSOP-14","NXP Semiconductors","74LVC06APW,118","Digi-Key","568-4490-1-ND",63,29.53]
["105","Voltage Level Translator Driver ","U25",1,"1","TXS0206-29","WCSP - YFP","Texas Instruments","TXS0206-29YFPR","Digi-Key","296-25577-1-ND",210,147.15]
["106","JK-FF","U26",1,"1","SN74LVC112APWR","TSSOP-16","Texas Instruments","SN74LVC112APWR","chip 1 stop","SN74LVC112APWR",null,null,"Digi-Key","296-8450-1-ND",79,54.05]
["107","Reset IC","U27",1,"1","TPS3808","SOT-23 DBV","Texas Instruments","TPS3808G12DBVR","Digi-Key","296-17190-1-ND",245,171.67,"chip1stop","TPS3808G12DBVR"]
["108","Dual Supply Bus Transceiver","U28,U29",2,"2","SN74AVCB164245VR","TVSOP-48","Texas Instruments","SN74AVCB164245VR","Digi-Key","296-15550-1-ND",420,308.31]
["109","Crystal　Oscillator","Y1",1,"1","SG-210SED",null,"Epson Toyocom","SG-210SEB","Tokyo Electron Device","SG-210SEB"]
["110","Crystal　Oscillator","Y2",1,"1","FX135",null,"FOX Electronics","FX135","Digi-Key","631-1002-1-ND",221,132.88]
["111","OMAP memory",null,1,"1",null,"FBGA",null,"MT29C4G48MAPLCJI-6"]