{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["bc10-005-0001_bom"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"bc10-005-0001_bom","index":0,"n_rows":59,"n_cols":20,"rows_kept":59,"cut":false,"hidden":false,"merged":[[1,3,1,7],[1,8,1,9],[1,10,1,11],[1,14,1,15],[3,0,8,0],[3,1,8,1],[3,8,8,8],[3,9,8,9],[3,10,8,10],[3,11,8,11],[3,12,8,12],[3,13,8,13],[3,14,8,14],[3,15,8,15],[3,16,8,16],[3,17,8,17],[3,18,8,18],[3,19,8,19],[9,0,13,0],[9,1,13,1],[9,8,13,8],[9,9,13,9],[9,10,13,10],[9,11,13,11],[9,12,13,12],[9,13,13,13],[9,14,13,14],[9,15,13,15],[9,16,13,16],[9,17,13,17],[9,18,13,18],[9,19,13,19],[15,0,16,0],[15,1,16,1],[15,8,16,8],[15,9,16,9],[15,10,16,10],[15,11,16,11],[15,12,16,12],[15,13,16,13],[15,14,16,14],[15,15,16,15],[15,16,16,16],[15,17,16,17],[15,18,16,18],[15,19,16,19],[23,0,24,0],[23,1,24,1],[23,8,24,8],[23,9,24,9],[23,10,24,10],[23,11,24,11],[23,12,24,12],[23,13,24,13],[23,14,24,14],[23,15,24,15],[23,16,24,16],[23,17,24,17],[23,18,24,18],[23,19,24,19],[26,0,27,0],[26,1,27,1],[26,8,27,8],[26,9,27,9],[26,10,27,10],[26,11,27,11],[26,12,27,12],[26,13,27,13],[26,14,27,14],[26,15,27,15],[26,16,27,16],[26,17,27,17],[26,18,27,18],[26,19,27,19],[29,0,32,0],[29,1,32,1],[29,8,32,8],[29,9,32,9],[29,10,32,10],[29,11,32,11],[29,12,32,12],[29,13,32,13],[29,14,32,14],[29,15,32,15],[29,16,32,16],[29,17,32,17],[29,18,32,18],[29,19,32,19],[34,0,45,0],[34,1,45,1],[34,8,45,8],[34,9,45,9],[34,10,45,10],[34,11,45,11],[34,12,45,12],[34,13,45,13],[34,14,45,14],[34,15,45,15],[34,16,45,16],[34,17,45,17],[34,18,45,18],[34,19,45,19],[46,0,52,0],[46,1,52,1],[46,8,52,8],[46,9,52,9],[46,10,52,10],[46,11,52,11],[46,12,52,12],[46,13,52,13],[46,14,52,14],[46,15,52,15],[46,16,52,16],[46,17,52,17],[46,18,52,18],[46,19,52,19]],"flags":["formulas_cached_only"]}
[{"$nulls":12},"Retailer Information"]
[null,null,null,"Mount Information",{"$nulls":4},"Component Information",null,"Component Maker Information",null,null,null,"Price (¥: Reference)",null,null,null,"参考価格"]
["項","Type","Reference","X-axis","Y-axis","Rotation","Surface\nMount","Mount","Description","Package","Maker","Product Number","Retailer1","Part Number","@mini  number unit per order ","@100 units","販売店2","販売店品番2","最小発注","100台分"]
["1","Ceramic Capacitor","C2",4.08,27.36,180,"Component","Required","0.1uF","1608","Murata","GRM188R71C104KA01D","Digi-Key","490-1532-1-ND",1.7,0.574]
[null,null,"C3",10.52,18.06,90,"Component","Required"]
[null,null,"C4",4.16,19.92,180,"Component","Required"]
[null,null,"C9",5.96,38.74,180,"Component","Required"]
[null,null,"C10",20.4,54.12,0,"Component","Required"]
[null,null,"C11",23.16,60.04,0,"Component","Required"]
["2","Ceramic Capacitor","C1",3.86,30.14,180,"Component","Required","22uF","2012","TAIYO YUDEN","LMK212BJ226MG-T","Digi-Key","587-1958-1-ND",92,34.45]
[null,null,"C5",3.96,17.46,180,"Component","Required"]
[null,null,"C6",16.34,22.1,0,"Component","Required"]
[null,null,"C7",12.32,22.06,180,"Component","Required"]
[null,null,"C8",5.58,41.52,180,"Component","Required"]
["3","Tantalum Capacitor","C12",4.84,12.02,180,"Component","Required","470uF","7260-35","Nichicon","F751A477MRC","Digi-Key","493-3372-1-ND"]
["4","Green LED","D2",24.12,62.9,90,"Component","Required","LG L29K-G2J1-24-Z","1608","OSRAM Opto Semiconductors Inc","LG L29K-G2J1-24-Z","Digi-Key","475-2709-1-ND",15,10.46]
[null,null,"D3",26.78,62.92,90,"Component","Required"]
["5","Diode","D1",15.9,57.74,0,"Component","Required","PGB1010603MR","1608","Littelfuse Inc","PGB1010603MR","Digi-Key","F2594CT-ND",49,37.47]
["6","6-Pin Connector","J1",16.8,6.3,0,"Component","Required","DF13A-6","DF13A-6","Hirose Electric Co Ltd","DF13A-6P-1.25H(20)","Digi-Key","H3371-ND",69,40.91]
["7","Expansion Connector","J2",27.2,37,90,"Component","Required","14 5078 030 510 861+",null,"KYOCERA　ELCO","14 5078 030 510 861+","Leocom","14 5078 030 510 861+",670,570,"チップワンストップ","145078030510861+",1100,658]
["8","Inductor","L1",10.42,40.28,270,"Component","Required","2.2μH",null,"TDK","VLF5014ST-2R2M2R3","Digi-Key","445-4238-1-ND",143,110.53]
["9","miniUSB TypeB","P1",15,65.9,180,"Component","Required","UX60 Series","USB miniB","Hirose Electric Co Ltd","UX60SC-MB-5ST(80)","Digi-Key","H11671CT-ND",91,53.83]
["10","Chip Resistor","R1",8.24,18.06,90,"Component","Required","60.4k","1608","Panasonic - ECG","ERJ-3EKF6042V","Digi-Key","P60.4KHCT-ND",4,1.09]
["11","Chip Resistor","R2",10.5,14.36,270,"Component","Required","30.1k","1608","Panasonic - ECG","ERJ-3EKF3012V","Digi-Key","P30.1KHCT-ND",4,1.09]
[null,null,"R10",27.3,54.45,180,"Component","Required"]
["12","Chip Resistor","R3",11.64,56.08,0,"Component","Required","330","1608","Panasonic - ECG","ERJ-3EKF3300V","Digi-Key","P330HCT-ND",4,1.09]
["13","Chip Resistor","R4",22.08,62.9,90,"Component","Required","1.5k","1608","Panasonic - ECG","ERJ-3EKF1501V","Digi-Key","P1.50KHCT-ND",4,1.09]
[null,null,"R8",27.32,60.1,0,"Component","Required"]
["14","Chip Resistor","R5",7.38,27.92,270,"Component","Required","20k","1608","Panasonic - ECG","ERJ-3EKF2002V","Digi-Key","P20.0KHCT-ND",4,1.09,"Digi-Key","RMCF0603FT20K0TR-ND"]
["15","Chip Resistor","R6",9.46,27.9,90,"Component","Required","10k","1608","Yageo","RC0603FR-0710KL","Digi-Key","311-10.0KHRCT-ND",6.4,1.995]
[null,null,"R7",11.56,27.9,90,"Component","Required"]
[null,null,"R11",17.92,26.34,180,"Component","Required"]
[null,null,"R12",21.35,25.85,180,"Component","Required"]
["16","Chip Resistor","R9",27.3,"56.,5",180,"Component","Required","174k","1608","Panasonic - ECG","ERJ-3EKF1743V","Digi-Key","P174KHCT-ND",4,1.09]
["17","Chip Resistor","R13",17.96,28.46,180,"Component","Not Required","0Ω","1608","Yageo","RC0603JR-070RL","Digi-Key","311-0.0GRCT-ND",6.1,1.91,"Digi-Key","RMCF0603ZT0R00CT-ND",2,0.368]
[null,null,"R14",21.28,29.34,180,"Component","Not Required"]
[null,null,"R15",21.28,39.76,180,"Component","Not Required"]
[null,null,"R16",16.66,40.96,180,"Component","Not Required"]
[null,null,"R17",21.28,41.86,180,"Component","Not Required"]
[null,null,"R18",18.88,44.12,180,"Component","Not Required"]
[null,null,"R21",17.1,31.28,180,"Component","Required"]
[null,null,"R22",21.28,31.86,180,"Component","Required"]
[null,null,"R23",21.3,35.48,180,"Component","Required"]
[null,null,"R24",16.94,34.82,180,"Component","Required"]
[null,null,"R25",21.26,37.66,180,"Component","Required"]
[null,null,"R26",16.9,36.96,180,"Component","Required"]
["18","Dome Switch","S1",23.5,24.5,0,"Soldering","Not Required","B3DA",null,"omron","B3DA","Digi-Key","SW1018-ND",276,248.36]
[null,null,"S2",23.5,41.5,0,"Soldering","Not Required"]
[null,null,"S5",15,16,270,"Soldering","Not Required"]
[null,null,"S6",15,33,270,"Soldering","Not Required"]
[null,null,"S7",15,50,90,"Soldering","Not Required"]
[null,null,"S9",6.5,24.5,180,"Soldering","Not Required"]
[null,null,"S10",6.5,41.5,180,"Soldering","Not Required"]
["19","Relay","U1",7.44,49.96,270,"Component","Required","AQV252G",null,"Panasonic Electric Works","AQV252GA","Digi-Key","255-1954-ND",537,372.56]
["20","Power Supply IC","U2",8.82,34.2,180,"Component","Required","TPS2500",null,"Texas Instruments","TPS2500DRCR","Digi-Key","296-25150-1-ND",345,252.65,"チップワンストップ","TPS2500DRCT",875,310]
["21","Power Supply IC","U3",5.82,23.5,0,"Component","Required","TPS73701",null,"Texas Instruments","TPS73701DRBR","Digi-Key","296-22065-1-ND",201,140.68]
["22","Voltage Supervisor","U4",22.18,57.06,90,"Component","Required","TL7700",null,"Texas Instruments","TL7700CDGKR","Digi-Key","296-24463-1-ND",359,263.18]
["23","Connector Socket Housing",{"$nulls":5},"Not Required","DF13-6S-1.25C",null,"Hirose Electric Co Ltd","DF13-6S-1.25C","Digi-Key","H2183-ND","30","10.53"]
["24","Connector Contact",{"$nulls":5},"Not Required","DF13-2630SCF",null,"Hirose Electric Co Ltd","DF13-2630SCF","Digi-Key","H9992CT-ND","12","1.684"]